Follow-On Topics

Related Topics

# Connecting to a Tobit Fax Server

King Task Centre supports Tobit FaxWare and Tobit David for use with the Send Fax (Tobit) tool. For any user to create a new Send Fax (Tobit) step the name of the DvISE Server to be used must first be specified through the Global Configuration dialog box.

## Adding a New Connection

1. You open the Send Fax (Tobit) global configuration by either:

|  | Going to Manage > Tools > Output > Send Fax (Tobit)

|  | From the , expanding King Task Centre > System > Tools > Output and double-clicking Send Fax (Tobit) in the

1. Enter the fax server's hostname into DvISE Server name. The default fax server name is "David".
2. You should also have a modem connected to your network with a spare license for a King Task Centre user account. For more information, refer to your Tobit documentation.

Copyright © 2018 Quadrant Software B.V. All rights reserved.